{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["探头编号","温度","湿度℃","坐标","记录时间"]
[2,3.8,54.4,"109.2730178833,27.743095397949","2024-09-14 09:54:00"]
[2,3.9,55.8,"109.2730178833,27.743095397949","2024-09-14 09:24:00"]
[2,4,53.8,"109.2730178833,27.743095397949","2024-09-14 08:54:00"]
[2,4.4,54.1,"109.2730178833,27.743095397949","2024-09-14 08:24:00"]
[2,4.8,54.9,"109.2730178833,27.743095397949","2024-09-14 07:54:00"]
[2,5.3,53.8,"109.2730178833,27.743095397949","2024-09-14 07:24:00"]
[2,5.8,50,"109.2730178833,27.743095397949","2024-09-14 06:54:00"]
[2,3.9,53.6,"109.2730178833,27.743095397949","2024-09-14 06:24:00"]
[2,4,54,"109.2730178833,27.743095397949","2024-09-14 05:54:00"]
[2,4.3,54.2,"109.2730178833,27.743095397949","2024-09-14 05:24:00"]
[2,4.7,54.7,"109.2730178833,27.743095397949","2024-09-14 04:54:00"]
[2,5,55.3,"109.2730178833,27.743095397949","2024-09-14 04:24:00"]
[2,6.2,49.7,"109.2730178833,27.743095397949","2024-09-14 03:54:00"]
[2,4.9,51.8,"109.2730178833,27.743095397949","2024-09-14 03:24:00"]
[2,3.8,54.1,"109.2730178833,27.743095397949","2024-09-14 02:54:00"]
[2,4.2,54.2,"109.2730178833,27.743095397949","2024-09-14 02:24:00"]
[2,4.3,54.5,"109.2730178833,27.743095397949","2024-09-14 01:54:00"]
[2,4.8,55.1,"109.2730178833,27.743095397949","2024-09-14 01:24:00"]
[2,5.2,54.6,"109.2730178833,27.743095397949","2024-09-14 00:54:00"]
[2,5.7,50.4,"109.2730178833,27.743095397949","2024-09-14 00:24:00"]