{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":4,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
["探头编号","温度℃","湿度%","记录时间"]
[1,17.3,53.5,"2024-06-07T10:06:23"]
[1,17.3,53.5,"2024-06-07T10:06:23"]
[1,17,56.4,"2024-06-07T10:05:23"]
[1,16.9,55.8,"2024-06-07T10:05:23"]
[1,17.4,55.3,"2024-06-07T10:04:53"]
[1,17,52.3,"2024-06-07T10:04:53"]
[1,17,51.7,"2024-06-07T10:04:20"]
[1,16.9,51.6,"2024-06-07T10:04:20"]
[1,17,51.9,"2024-06-07T10:03:44"]
[1,17,52.8,"2024-06-07T10:03:44"]
[1,16.9,52,"2024-06-05T17:11:23"]
[1,16.9,52.1,"2024-06-05T17:11:23"]
[1,17,52.1,"2024-06-05T17:11:00"]
[2,16.8,50.7,"2024-06-05T17:11:00"]
[2,16.9,50.8,"2024-06-05T17:07:10"]
[2,17,51,"2024-06-05T17:07:10"]
[2,16.9,51.1,"2024-06-05T17:00:58"]
[2,16.9,51.2,"2024-06-05T17:00:58"]
[2,17,51,"2024-06-05T16:56:53"]
[2,16.9,51.3,"2024-06-05T16:56:53"]
[2,17,51.4,"2024-06-05T16:50:51"]
[2,16.9,51.4,"2024-06-05T16:50:51"]
[2,16.9,51.4,"2024-06-05T16:50:35"]
[2,16.9,51.6,"2024-06-05T16:50:35"]
[3,17,51.7,"2024-06-05T16:50:18"]
[3,17,51.9,"2024-06-05T16:50:18"]
[3,17.1,51.8,"2024-06-05T16:50:02"]
[3,17.1,52.1,"2024-06-05T16:50:02"]
[3,17.1,52.1,"2024-06-05T16:49:40"]